Настройка двух мониторов под МСВС

Авансцена: ноутбук Т60. видеоплата ATI Mobility Radeon x1400, МСВС 3.0 сборка 13

Проблема: кнопка Fn+F7 переключает либо на внешний монитор, либо на локальный, а хочется, чтобы оператор смотрел не на проектор, а на локальный монитор

1. Скачал драйвер отсюда http://ati.amd.com/support/drivers/linux/linux-radeon.html

2. При запуске ati-driver-installer-8.36.5-x86.x86_64.run ругается так

[root@mdbc_v13 root]# ./ati-driver-installer-8.36.5-x86.x86_64.run
Created directory fglrx-install.ojSEbb
Verifying archive integrity... All good.
Uncompressing ATI Proprietary Linux Driver-8.36.5.........................................................
..........................................................................................................
..........................................................................................................
..........................................................................................................
..........................................................................................................
..........................................................................................................
....................................................
==================================================
ATI Technologies Linux Driver Installer/Packager
==================================================
mktemp: invalid option -- t
Usage: mktemp [-d] [-q] [-u] template
mktemp: invalid option -- t
Usage: mktemp [-d] [-q] [-u] template
./ati-installer.sh: line 158: $OUT_FILE: ambiguous redirect
./ati-installer.sh: line 169: $OUT_FILE: ambiguous redirect
./ati-installer.sh: line 659: .: filename argument required
.: usage: . filename
Removing temporary directory: fglrx-install.ojSEbb

3. Разархивировал в каталог ATI

./ati-driver-installer-8.36.5-x86.x86_64.run --extract ATI

4. Внутри ATI в файле ati-installer.sh удалил из строче вызова mktemp ключ -t потом выяснилось, что установка все равно не работает

5. Скопировал файлы подкаталога x680 (для версии xorg 6.8.x) в дерево X11

6. Исправил xorg.conf так

# File generated by OC MCBC 3.0 installer.
Section "ServerLayout"
Identifier "Anaconda Configured"
Screen 0 "Screen0" 0 0
InputDevice "Mouse0" "CorePointer"
InputDevice	"Mouse1" "SendCoreEvents"
InputDevice "Keyboard0" "CoreKeyboard"
# !!! uncoment to use Ctrl+Alt+Baclspace !!!
#	Option	"DontZap"	"False"
EndSection
Section "Files"
# The location of the RGB database. Note, this is the name of the
# file minus the extension (like ".txt" or ".db"). There is normally
# no need to change the default.
RgbPath	"/usr/X11R6/lib/X11/rgb"
# Multiple FontPath entries are allowed (they are concatenated together)
# By default, Red Hat 6.0 and later now use a font server independent of
# the X server to render fonts.
FontPath "unix/:7100"
EndSection
Section "Module"
Load "dbe"
Load "extmod"
Load "fbdevhw"
Load "dri"
Load "glx"
Load "record"
Load "freetype"
Load "type1"
EndSection
Section "InputDevice"
Identifier "Keyboard0"
Driver "keyboard"
#	Option	"AutoRepeat"	"500 5"
# when using XQUEUE, comment out the above line, and uncomment the
# following line
#	Option	"Protocol"	"Xqueue"
# Specify which keyboard LEDs can be user-controlled (eg, with xset(1))
#	Option	"Xleds"	"1 2 3"
# To disable the XKEYBOARD extension, uncomment XkbDisable.
#	Option	"XkbDisable"
# To customise the XKB settings to suit your keyboard, modify the
# lines below (which are the defaults). For example, for a non-U.S.
# keyboard, you will probably want to use:
#	Option	"XkbModel"	"pc102"
# If you have a US Microsoft Natural keyboard, you can use:
#	Option	"XkbModel"	"microsoft"
#
# Then to change the language, change the Layout setting.
# For example, a german layout can be obtained with:
#	Option	"XkbLayout"	"de"
# or:
#	Option	"XkbLayout"	"de"
#	Option	"XkbVariant"	"nodeadkeys"
#
# If you'd like to switch the positions of your capslock and
# control keys, use:
#	Option	"XkbOptions"	"ctrl:swapcaps"
Option	"XkbRules"	"xfree86"
Option	"XkbModel"	"pc102"
Option	"XkbLayout"	"us,ru"
#Option	"XkbVariant"	"basic,winkeys"
Option	"XkbOptions"	"grp:ctrl_shift_toggle"
EndSection
Section "InputDevice"
Identifier "Mouse0"
Driver "mouse"
Option "Protocol" "PS/2"
Option "Device" "/dev/psaux"
# Option "ZAxisMapping" "4 5"
Option "Emulate3Buttons" "no"
EndSection
Section "InputDevice"
Identifier	"Mouse1"
Driver	"mouse"
Option	"Device"	"/dev/input/mice"
Option	"Protocol"	"PS/2"
Option	"Emulate3Buttons"	"no"
Option	"ZAxisMapping"	"4 5"
EndSection
Section "Monitor"
Identifier "Monitor0"
VendorName "Неопределенный монитор"
ModelName "Неопределенный монитор"
HorizSync 31.5-80.5
VertRefresh 50-90
# Option "dpms"
EndSection
Section "Monitor"
Identifier "Monitor1"
VendorName "Неопределенный монитор"
ModelName "Неопределенный монитор"
HorizSync 31.5-80.5
VertRefresh 50-90
# Option "dpms"
EndSection
Section "Device"
# no known options
Identifier "ati"
Driver "fglrx"
VendorName "vesa"
BoardName "VESA driver (generic)"
# Option "Clone" "true"
#	Option "MonitorLayout" "CRT,LFP"
#	Option "ShadowFB" "off"
# BusID "PCI:1:0:0"
EndSection
Section "Screen"
Identifier "Screen0"
Device "ati"
Monitor "Monitor0"
DefaultDepth	24
Subsection "Display"
Depth 24
Modes "1280x1024" "1024x768" "800x600" "640x480"
EndSubsection
EndSection
Section "DRI"
Mode 0666
EndSection