802.11s mesh powersaving for linux

Plan

find out what's to be done

find out how analogous things are done

do it

What's to be done

MSTA power mode tracking (11C.13.3);

each peering power mode tracking (11C.13.4);

TIM/DTIM in beacons (11C.13.5-6) – ieee80211_beacon_get_tim;

mesh awake window (11C.13.7);

wake-up scheduling for peer beacons (optional);

ps-poll requests and responses (?);

service period tracking (11C.13.10);

frame buffering for peers in doze state;